(footprint "Samtec_HSEC8-109-X-X-DV-BL_2x09_P0.8mm_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge for PCB's with 2x9 contacts (with board lock option)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -7.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-109-X-X-DV-BL_2x09_P0.8mm_Edge"
		(at 0 0.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -10.325 -6)
		(end -10.325 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -9.925 -7.78)
		(end -7.325 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -6.825 -6)
		(end -10.325 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.825 -5)
		(end -5.825 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.825 0)
		(end -1.595 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.595 0)
		(end -1.595 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0.805 -5.2)
		(end 0.805 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0.805 0)
		(end 5.825 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.825 0)
		(end 5.825 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 6.825 -6)
		(end 10.325 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 9.925 -7.78)
		(end 7.325 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.325 -6)
		(end 10.325 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -10.325 -7.38)
		(mid -10.207843 -7.662843)
		(end -9.925 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -6.825 -6)
		(mid -6.117893 -5.707107)
		(end -5.825 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -6.325 -8.78)
		(mid -6.617893 -8.072893)
		(end -7.325 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -1.595 -5.2)
		(mid -0.395 -6.4)
		(end 0.805 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 5.825 -5)
		(mid 6.117893 -5.707107)
		(end 6.825 -6)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 7.325 -7.78)
		(mid 6.617893 -8.072893)
		(end 6.325 -8.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 9.925 -7.78)
		(mid 10.207843 -7.662843)
		(end 10.325 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_text user "1"
		(at -4.8 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "17"
		(at 4.425 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "7"
		(at -2.4 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "9"
		(at 1.6 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "10"
		(at 1.975 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "18"
		(at 4.425 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "2"
		(at -4.8 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "8"
		(at -2.4 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "Chamfer 30 degree 0.45 mm"
		(at 0 -0.44 0)
		(layer "Cmts.User")
	)
	(fp_text user "mated PCB distance: 1.80 mm (ref)"
		(at -3.08 1.8 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -4.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -4.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -3.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -3.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -2.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -2.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at 1.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at 1.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at 2.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at 2.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at 3.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at 3.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at 4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at 4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at 4.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at 4.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
