(footprint "Samtec_HSEC8-110-X-X-DV_2x10_P0.8mm_Wing_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge for PCB's with 2x10 contacts (with horizontal Edge.Cuts ends)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -7.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-110-X-X-DV_2x10_P0.8mm_Wing_Edge"
		(at 0 0.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -4.625 -5)
		(end -4.625 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.625 0)
		(end 4.625 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.625 0)
		(end 4.625 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -5.625 -6)
		(mid -4.917893 -5.707107)
		(end -4.625 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 4.625 -5)
		(mid 4.917893 -5.707107)
		(end 5.625 -6)
		(layer "Edge.Cuts")
	)
	(fp_text user "19"
		(at 3.225 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -3.6 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "20"
		(at 3.225 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "2"
		(at -3.6 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "Chamfer 30 degree 0.45 mm"
		(at 0 -0.44 0)
		(layer "Cmts.User")
	)
	(fp_text user "mated PCB distance: 3.69 mm (max)"
		(at -1.88 3.69 0)
		(layer "Cmts.User")
	)
	(fp_text user "mated PCB distance: 2.05 mm (min)"
		(at -1.88 2.05 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -3.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -3.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -2.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -2.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -1.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -1.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -0.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at -0.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at 0.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at 0.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at 1.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at 1.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at 2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at 2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at 2.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at 2.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at 3.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at 3.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
