(footprint "Samtec_HSEC8-113-01-X-DV-A-WT_2x13_P0.8mm_Pol06_Socket_WeldTabs"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0.8 mm Highspeed card edge card connector socket for 1.57mm PCBs, vertical, alignment pins, weld tabs (source: https://suddendocs.samtec.com/prints/hsec8-1xxx-xx-xx-dv-x-xx-footprint.pdf)")
	(tags "conn samtec card-edge socket high-speed")
	(property "Reference" "REF**"
		(at 0 -4.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-113-01-X-DV-A-WT_2x13_P0.8mm_Pol06_Socket_WeldTabs"
		(at 0 4.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -10.25 0)
		(size 2.54 2.54)
		(drill 0.84)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "" np_thru_hole circle
		(at -7.9 1.5)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.9 0)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" thru_hole circle
		(at 10.25 0)
		(size 2.54 2.54)
		(drill 0.84)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "1" smd roundrect
		(at -6.4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -6.4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -5.6 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -5.6 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.8 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.8 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.2 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.2 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -2.4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -2.4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.6 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.6 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 3.2 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 3.2 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 4.8 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 4.8 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 5.6 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 5.6 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 6.4 1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 6.4 -1.7)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HSEC8.3dshapes/Samtec_HSEC8-113-01-X-DV-A-WT_2x13_P0.8mm_Pol06_Socket_WeldTabs.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
