(footprint "Samtec_HSEC8-125-X-X-DV-BL_2x25_P0.8mm_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge for PCB's with 2x25 contacts (with board lock option)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -7.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-125-X-X-DV-BL_2x25_P0.8mm_Edge"
		(at 0 0.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -16.725 -6)
		(end -16.725 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -16.325 -7.78)
		(end -13.725 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -13.225 -6)
		(end -16.725 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -12.225 -5)
		(end -12.225 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -12.225 0)
		(end -6.395 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -6.395 0)
		(end -6.395 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.995 -5.2)
		(end -3.995 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.995 0)
		(end 12.225 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.225 0)
		(end 12.225 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 13.225 -6)
		(end 16.725 -6)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 16.325 -7.78)
		(end 13.725 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 16.725 -6)
		(end 16.725 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -16.725 -7.38)
		(mid -16.607843 -7.662843)
		(end -16.325 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -13.225 -6)
		(mid -12.517893 -5.707107)
		(end -12.225 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -12.725 -8.78)
		(mid -13.017893 -8.072893)
		(end -13.725 -7.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -6.395 -5.2)
		(mid -5.195 -6.4)
		(end -3.995 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 12.225 -5)
		(mid 12.517893 -5.707107)
		(end 13.225 -6)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 13.725 -7.78)
		(mid 13.017893 -8.072893)
		(end 12.725 -8.78)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 16.325 -7.78)
		(mid 16.607843 -7.662843)
		(end 16.725 -7.38)
		(layer "Edge.Cuts")
	)
	(fp_text user "49"
		(at 10.825 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "13"
		(at -2.825 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "11"
		(at -7.575 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -11.2 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "50"
		(at 10.825 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "14"
		(at -2.825 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "2"
		(at -11.2 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "12"
		(at -7.575 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "Chamfer 30 degree 0.45 mm"
		(at 0 -0.44 0)
		(layer "Cmts.User")
	)
	(fp_text user "mated PCB distance: 1.80 mm (ref)"
		(at -9.48 1.8 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -11.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -11.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -10.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -10.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -9.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -9.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -8.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -8.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at -8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at -7.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at -7.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at -3.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at -3.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at -2.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at -2.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -1.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at -1.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -0.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at -0.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at 0 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" connect rect
		(at 0 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at 0.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" connect rect
		(at 0.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at 1.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" connect rect
		(at 1.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at 2.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" connect rect
		(at 2.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at 3.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" connect rect
		(at 3.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at 4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" connect rect
		(at 4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "33" connect rect
		(at 4.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at 4.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "35" connect rect
		(at 5.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at 5.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "37" connect rect
		(at 6.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at 6.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "39" connect rect
		(at 7.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at 7.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "41" connect rect
		(at 8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at 8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "43" connect rect
		(at 8.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at 8.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "45" connect rect
		(at 9.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at 9.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "47" connect rect
		(at 10.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at 10.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "49" connect rect
		(at 11.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at 11.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
