(footprint "Samtec_HSEC8-170-X-X-DV_2x70_P0.8mm_Wing_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge for PCB's with 2x70 contacts (with horizontal Edge.Cuts ends)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -7.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-170-X-X-DV_2x70_P0.8mm_Wing_Edge"
		(at 0 0.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -30.225 -5)
		(end -30.225 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -30.225 0)
		(end -3.595 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.595 0)
		(end -3.595 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.195 -5.2)
		(end -1.195 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.195 0)
		(end 30.225 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 30.225 0)
		(end 30.225 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -31.225 -6)
		(mid -30.517893 -5.707107)
		(end -30.225 -5)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -3.595 -5.2)
		(mid -2.395 -6.4)
		(end -1.195 -5.2)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 30.225 -5)
		(mid 30.517893 -5.707107)
		(end 31.225 -6)
		(layer "Edge.Cuts")
	)
	(fp_text user "139"
		(at 28.45 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -29.2 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "63"
		(at -4.775 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "65"
		(at -0.025 -4.55 0)
		(layer "F.SilkS")
	)
	(fp_text user "140"
		(at 28.45 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "64"
		(at -4.775 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "66"
		(at -0.025 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "2"
		(at -29.2 -4.55 0)
		(layer "B.SilkS")
	)
	(fp_text user "mated PCB distance: 2.05 mm (min)"
		(at -27.48 2.05 0)
		(layer "Cmts.User")
	)
	(fp_text user "mated PCB distance: 3.69 mm (max)"
		(at -27.48 3.69 0)
		(layer "Cmts.User")
	)
	(fp_text user "Chamfer 30 degree 0.45 mm"
		(at 0 -0.44 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -29.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -29.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -28.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -28.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -27.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -27.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -26.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -26.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -26 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at -26 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at -25.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at -25.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at -24.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at -24.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at -23.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at -23.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -22.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at -22.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -22 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at -22 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at -21.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" connect rect
		(at -21.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at -20.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" connect rect
		(at -20.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at -19.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" connect rect
		(at -19.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at -18.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" connect rect
		(at -18.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at -18 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" connect rect
		(at -18 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at -17.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" connect rect
		(at -17.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "33" connect rect
		(at -16.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at -16.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "35" connect rect
		(at -15.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at -15.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "37" connect rect
		(at -14.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at -14.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "39" connect rect
		(at -14 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at -14 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "41" connect rect
		(at -13.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at -13.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "43" connect rect
		(at -12.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at -12.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "45" connect rect
		(at -11.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at -11.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "47" connect rect
		(at -10.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at -10.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "49" connect rect
		(at -10 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at -10 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "51" connect rect
		(at -9.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at -9.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "53" connect rect
		(at -8.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at -8.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "55" connect rect
		(at -7.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at -7.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "57" connect rect
		(at -6.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at -6.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "59" connect rect
		(at -6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at -6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "61" connect rect
		(at -5.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" connect rect
		(at -5.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "63" connect rect
		(at -4.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "64" connect rect
		(at -4.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "65" connect rect
		(at -0.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "66" connect rect
		(at -0.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "67" connect rect
		(at 0.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "68" connect rect
		(at 0.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "69" connect rect
		(at 1.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "70" connect rect
		(at 1.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "71" connect rect
		(at 2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "72" connect rect
		(at 2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "73" connect rect
		(at 2.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "74" connect rect
		(at 2.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "75" connect rect
		(at 3.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "76" connect rect
		(at 3.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "77" connect rect
		(at 4.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "78" connect rect
		(at 4.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "79" connect rect
		(at 5.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "80" connect rect
		(at 5.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "81" connect rect
		(at 6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" connect rect
		(at 6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "83" connect rect
		(at 6.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" connect rect
		(at 6.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "85" connect rect
		(at 7.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" connect rect
		(at 7.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "87" connect rect
		(at 8.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" connect rect
		(at 8.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "89" connect rect
		(at 9.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" connect rect
		(at 9.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "91" connect rect
		(at 10 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" connect rect
		(at 10 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "93" connect rect
		(at 10.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" connect rect
		(at 10.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "95" connect rect
		(at 11.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "96" connect rect
		(at 11.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "97" connect rect
		(at 12.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "98" connect rect
		(at 12.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "99" connect rect
		(at 13.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "100" connect rect
		(at 13.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "101" connect rect
		(at 14 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "102" connect rect
		(at 14 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "103" connect rect
		(at 14.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "104" connect rect
		(at 14.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "105" connect rect
		(at 15.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "106" connect rect
		(at 15.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "107" connect rect
		(at 16.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "108" connect rect
		(at 16.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "109" connect rect
		(at 17.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "110" connect rect
		(at 17.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "111" connect rect
		(at 18 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "112" connect rect
		(at 18 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "113" connect rect
		(at 18.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "114" connect rect
		(at 18.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "115" connect rect
		(at 19.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "116" connect rect
		(at 19.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "117" connect rect
		(at 20.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "118" connect rect
		(at 20.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "119" connect rect
		(at 21.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "120" connect rect
		(at 21.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "121" connect rect
		(at 22 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "122" connect rect
		(at 22 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "123" connect rect
		(at 22.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "124" connect rect
		(at 22.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "125" connect rect
		(at 23.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "126" connect rect
		(at 23.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "127" connect rect
		(at 24.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "128" connect rect
		(at 24.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "129" connect rect
		(at 25.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "130" connect rect
		(at 25.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "131" connect rect
		(at 26 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "132" connect rect
		(at 26 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "133" connect rect
		(at 26.8 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "134" connect rect
		(at 26.8 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "135" connect rect
		(at 27.6 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "136" connect rect
		(at 27.6 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "137" connect rect
		(at 28.4 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "138" connect rect
		(at 28.4 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(pad "139" connect rect
		(at 29.2 -2.4)
		(size 0.55 2.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "140" connect rect
		(at 29.2 -2.4)
		(size 0.55 2.8)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
