(footprint "Samtec_HSEC8-180-03-X-DV_2x80_P0.8mm_Pol32_Socket"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0.8 mm Highspeed card edge card connector socket for 2.36mm PCBs, vertical (source: https://suddendocs.samtec.com/prints/hsec8-1xxx-xx-xx-dv-x-xx-footprint.pdf)")
	(tags "conn samtec card-edge socket high-speed")
	(property "Reference" "REF**"
		(at 0 -5.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HSEC8-180-03-X-DV_2x80_P0.8mm_Pol32_Socket"
		(at 0 5.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -33.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -33.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -32.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -32.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -31.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -31.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -30.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -30.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -30 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -30 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -29.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -29.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -28.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -28.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -27.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -27.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -26.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -26.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -26 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -26 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -25.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -25.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -24.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -24.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -23.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -23.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -22.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -22.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -22 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -22 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -21.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -21.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -20.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -20.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -19.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -19.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -18.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -18.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -18 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -18 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -17.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at -17.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -16.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -16.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at -15.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at -15.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -14.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -14.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at -14 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -14 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -13.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -13.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -12.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -12.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at -11.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at -11.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at -10.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at -10.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at -10 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at -10 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at -9.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at -9.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at -8.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at -8.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at -4.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at -4.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at -3.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at -3.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at -2.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at -2.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at -2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at -2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at -1.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at -1.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at -0.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at -0.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at 0.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at 0.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at 1.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at 1.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at 2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at 2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at 2.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at 2.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at 3.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at 3.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at 4.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at 4.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "89" smd roundrect
		(at 5.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "90" smd roundrect
		(at 5.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "91" smd roundrect
		(at 6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "92" smd roundrect
		(at 6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "93" smd roundrect
		(at 6.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "94" smd roundrect
		(at 6.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "95" smd roundrect
		(at 7.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "96" smd roundrect
		(at 7.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "97" smd roundrect
		(at 8.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "98" smd roundrect
		(at 8.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "99" smd roundrect
		(at 9.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "100" smd roundrect
		(at 9.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "101" smd roundrect
		(at 10 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "102" smd roundrect
		(at 10 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at 10.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "104" smd roundrect
		(at 10.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "105" smd roundrect
		(at 11.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "106" smd roundrect
		(at 11.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "107" smd roundrect
		(at 12.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "108" smd roundrect
		(at 12.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "109" smd roundrect
		(at 13.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "110" smd roundrect
		(at 13.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "111" smd roundrect
		(at 14 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "112" smd roundrect
		(at 14 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "113" smd roundrect
		(at 14.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "114" smd roundrect
		(at 14.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "115" smd roundrect
		(at 15.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "116" smd roundrect
		(at 15.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "117" smd roundrect
		(at 16.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "118" smd roundrect
		(at 16.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "119" smd roundrect
		(at 17.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "120" smd roundrect
		(at 17.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "121" smd roundrect
		(at 18 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "122" smd roundrect
		(at 18 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "123" smd roundrect
		(at 18.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "124" smd roundrect
		(at 18.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "125" smd roundrect
		(at 19.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "126" smd roundrect
		(at 19.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "127" smd roundrect
		(at 20.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "128" smd roundrect
		(at 20.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "129" smd roundrect
		(at 21.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "130" smd roundrect
		(at 21.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "131" smd roundrect
		(at 22 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "132" smd roundrect
		(at 22 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "133" smd roundrect
		(at 22.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "134" smd roundrect
		(at 22.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "135" smd roundrect
		(at 23.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "136" smd roundrect
		(at 23.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "137" smd roundrect
		(at 24.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "138" smd roundrect
		(at 24.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "139" smd roundrect
		(at 25.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "140" smd roundrect
		(at 25.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "141" smd roundrect
		(at 26 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "142" smd roundrect
		(at 26 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "143" smd roundrect
		(at 26.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "144" smd roundrect
		(at 26.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "145" smd roundrect
		(at 27.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "146" smd roundrect
		(at 27.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "147" smd roundrect
		(at 28.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "148" smd roundrect
		(at 28.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "149" smd roundrect
		(at 29.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "150" smd roundrect
		(at 29.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "151" smd roundrect
		(at 30 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "152" smd roundrect
		(at 30 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "153" smd roundrect
		(at 30.8 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "154" smd roundrect
		(at 30.8 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "155" smd roundrect
		(at 31.6 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "156" smd roundrect
		(at 31.6 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "157" smd roundrect
		(at 32.4 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "158" smd roundrect
		(at 32.4 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "159" smd roundrect
		(at 33.2 2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "160" smd roundrect
		(at 33.2 -2.095)
		(size 0.5 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HSEC8.3dshapes/Samtec_HSEC8-180-03-X-DV_2x80_P0.8mm_Pol32_Socket.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
