(footprint "Samtec_T1M-12-X-S-V_1x12-1MP_P1.0mm_Terminal_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Samtec Micro Mate Discrete Wire Terminal Strip, 1.00 mm Pitch, Single Row, Vertical (source: https://suddendocs.samtec.com/prints/t1m-single-row-footprint.pdf)")
	(tags "conn samtec discrete wire terminal")
	(property "Reference" "REF**"
		(at 0 -2.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_T1M-12-X-S-V_1x12-1MP_P1.0mm_Terminal_Vertical"
		(at 0 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 3.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 4.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 5.5 1.925)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -6.8 -0.6)
		(size 0.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 6.8 -0.6)
		(size 0.8 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_MicroMate.3dshapes/Samtec_T1M-12-X-S-V_1x12-1MP_P1.0mm_Terminal_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
