(footprint "Samtec_UMPS-04-XX.X-X-V-S_1x04_P2.0mm_Socket"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "2.00 mm mPOWER Ultra Micro Power Socket (source: https://suddendocs.samtec.com/prints/umps-xx-xx.x-xx-v-x-x-xr-footprint.pdf)")
	(tags "conn samtec ultra-mirco-power socket")
	(property "Reference" "REF**"
		(at 0 -4.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_UMPS-04-XX.X-X-V-S_1x04_P2.0mm_Socket"
		(at 0 4.3 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -3 0)
		(size 1.3 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1 0)
		(size 1.3 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1 0)
		(size 1.3 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 3 0)
		(size 1.3 3.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_MicroPower.3dshapes/Samtec_UMPS-04-XX.X-X-V-S_1x04_P2.0mm_Socket.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
