(footprint "TE_2834006-4_1x04_P4.0mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TE Connectivity Buchanan WireMate connector, Poke-In series, 4-way, 4.0mm pitch, AWG18-22 (0.3255-0.823mm2), https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F2834006%7FB6%7Fpdf%7FEnglish%7FENG_CD_2834006_B6.pdf%7F2834006-1")
	(tags "wire connector")
	(property "Reference" "REF**"
		(at 0 -8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "TE_2834006-4_1x04_P4.0mm_Horizontal"
		(at 0 7.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -2 1.5 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -6 -5.25)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -6 4)
		(size 2 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2 -5.25)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2 4)
		(size 2 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 2 -5.25)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 2 4)
		(size 2 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 6 -5.25)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 6 4)
		(size 2 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_2834006-4_1x04_P4.0mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
