(footprint "TE_440055-2_1x02_P2.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TE Connectivity, HDI, Wire-to-Board, Fully Shrouded, Header: https://www.te.com/usa-en/product-440055-2.datasheet.pdf")
	(tags "connector header hdr horizontal right-angle shrouded fully-shrounded 440055-2 2-440055-2 4-440055-2 6-440055-2 8-440055-2")
	(property "Reference" "REF**"
		(at 1 -2.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "TE_440055-2_1x02_P2.00mm_Horizontal"
		(at 1 9.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1 3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole oval
		(at 2 0)
		(size 1.2 1.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_440055-2_1x02_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
