(footprint "TE_5767171-1_2x19_P0.635mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCB Mount Receptacle, Vertical, Board-to-Board, 38 Position, 24.003mm / .64mm [.945in] Centerline, Header Only, Palladium Nickel (https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F5767171%7FB2%7Fpdf%7FEnglish%7FENG_CD_5767171_B2.pdf%7F5767171-1#page=2)")
	(tags "mictor38 receptacle board-to-board")
	(property "Reference" "REF**"
		(at 0 -14.1575 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_5767171-1_2x19_P0.635mm_Vertical"
		(at 0 14.5425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3.3575 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -11.44 90)
		(size 2.39 2.39)
		(drill 2.39)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -3.53 -5.725 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.53 -5.725 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.53 -5.09 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.53 -5.09 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.53 -4.455 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.53 -4.455 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.53 -3.82 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3.53 -3.82 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.53 -3.185 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.53 -3.185 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.53 -2.55 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 3.53 -2.55 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.53 -1.915 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 3.53 -1.915 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.53 -1.28 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 3.53 -1.28 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.53 -0.645 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 3.53 -0.645 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.53 -0.01 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 3.53 -0.01 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -3.53 0.625 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.53 0.625 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -3.53 1.26 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 3.53 1.26 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -3.53 1.895 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 3.53 1.895 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -3.53 2.53 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 3.53 2.53 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -3.53 3.165 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.53 3.165 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -3.53 3.8 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.53 3.8 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -3.53 4.435 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.53 4.435 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -3.53 5.07 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.53 5.07 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -3.53 5.705 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 3.53 5.705 180)
		(size 1.27 0.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole circle
		(at 0 -5.09 90)
		(size 1.318 1.318)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0 -2.55 90)
		(size 1.318 1.318)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0 -0.01 90)
		(size 1.318 1.318)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0 2.53 90)
		(size 1.318 1.318)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 0 5.07 90)
		(size 1.318 1.318)
		(drill 0.81)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_5767171-1_2x19_P0.635mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
