(footprint "TE_826576-7_1x07_P3.96mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TE, 826576-7, 7 Pins (https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=826576&DocType=Customer+Drawing&DocLang=English), generated with kicad-footprint-generator")
	(tags "connector TE 826576 vertical")
	(property "Reference" "REF**"
		(at 11.88 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_826576-7_1x07_P3.96mm_Vertical"
		(at 11.88 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.88 -2.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.104167)
	)
	(pad "2" thru_hole circle
		(at 3.96 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7.92 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 11.88 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 15.84 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 19.8 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 23.76 0)
		(size 2.4 2.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_826576-7_1x07_P3.96mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
