(footprint "TE_AMPSEAL_1-776087-x_3Rows_23_P0.4mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector")
	(tags "TE 776087")
	(property "Reference" "REF**"
		(at -7.6 1.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_AMPSEAL_1-776087-x_3Rows_23_P0.4mm_Horizontal"
		(at 30 11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PCB Edge"
		(at 14.4 13.55 0)
		(layer "Dwgs.User")
	)
	(fp_text user "Panel Edge"
		(at 14 16.55 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 14 4 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -6.5 4.5)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu")
	)
	(pad "" np_thru_hole circle
		(at 34.5 4.5)
		(size 2.85 2.85)
		(drill 2.85)
		(layers "*.Cu")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 4 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 8 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 12 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 16 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 20 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 24 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 28 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 6 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 10 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 14 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 18 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 22 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 26 4)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 0 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 4 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 8 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 12 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 16 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 20 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 24 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 28 8)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_AMPSEAL_1-776087-x_3Rows_23_P0.4mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
