(footprint "TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F350211%7FU5%7Fpdf%7FEnglish%7FENG_CD_350211_U5.pdf%7F350211-1")
	(tags "connector TE MATE-N-LOK top entry ATA PATA IDE 5.25 inch floppy drive power")
	(property "Reference" "REF**"
		(at 8.89 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical"
		(at 7.62 5.01 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.78 2.78)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.78 2.78)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 2.78 2.78)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 15.24 0)
		(size 2.78 2.78)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_MATE-N-LOK_350211-1_1x04_P5.08mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
