(footprint "TE_T4041037041-000_M8_04_Socket_Straight"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded M8 socket 4 ways connector panel, straight and rear mount (https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FT404103010X000%7FA%7Fpdf%7FEnglish%7FENG_CD_T404103010X000_A.pdf%7FT4041037041-000)")
	(tags "four-pin M8")
	(property "Reference" "REF**"
		(at 1.7 -8.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_T4041037041-000_M8_04_Socket_Straight"
		(at 1.75 8.72 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.75 0.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 17.8)
		(size 1.74 1.74)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0.625 1.95 180)
		(size 1.74 1.74)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.4 0 180)
		(size 1.74 1.74)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.775 1.95 180)
		(size 1.74 1.74)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -4.55 0.5 180)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 7.95 0.5 180)
		(size 5 5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_TE-Connectivity.3dshapes/TE_T4041037041-000_M8_04_Socket_Straight.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
