(footprint "USB3_A_Receptacle_Wuerth_692122030100"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB 3.0, type A, right angle (https://www.we-online.com/katalog/datasheet/692122030100.pdf)")
	(tags "USB 3.0 type A right angle Würth")
	(property "Reference" "REF**"
		(at 0 -10.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB3_A_Receptacle_Wuerth_692122030100"
		(at -0.05 -0.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.9 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.4 -3.45)
		(size 2 2)
		(drill 2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.4 -3.45)
		(size 2 2)
		(drill 2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -3.75 -8.67)
		(size 0.9 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.25 -8.67)
		(size 0.9 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1.25 -8.67)
		(size 0.9 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 3.75 -8.67)
		(size 0.9 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 5 -8.895)
		(size 0.9 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.5 -8.895)
		(size 0.9 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0 -8.895)
		(size 0.9 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.5 -8.895)
		(size 0.9 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -5 -8.895)
		(size 0.9 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" thru_hole oval
		(at -6.8 -3.45)
		(size 2.52 3.4)
		(drill oval 1.12 2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 6.8 -3.45)
		(size 2.52 3.4)
		(drill oval 1.12 2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB3_A_Receptacle_Wuerth_692122030100.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
