(footprint "USB_A_CNCTech_1001-011-01101_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
	(tags "USB-A")
	(property "Reference" "REF**"
		(at -6.9 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_CNCTech_1001-011-01101_Horizontal"
		(at 0 8 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at -4.55 -0.05 90)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -6 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -6.9 -2.3)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -6.9 2.3)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -9.65 -3.5)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9.65 -1)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -9.65 1)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -9.65 3.5)
		(size 2.5 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" thru_hole oval
		(at -6.9 -5.7)
		(size 3.5 1.9)
		(drill oval 2.5 0.9)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -6.9 5.7)
		(size 3.5 1.9)
		(drill oval 2.5 0.9)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
