(footprint "USB_A_Connfly_DS1098_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB type A Plug, Horizontal, https://en.connfly.com/static/upload/file//DS1098.pdf")
	(tags "USB-A")
	(property "Reference" "REF**"
		(at -8.3 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_Connfly_DS1098_Horizontal"
		(at 0 9 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at -4.3 0 90)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -8.3 -2.25)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.3 2.25)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Mask")
	)
	(pad "1" smd roundrect
		(at -10.55 -3.5)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -10.55 -1)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -10.55 1)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -10.55 3.5)
		(size 2.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" thru_hole oval
		(at -8.3 -5.85)
		(size 3.8 1.4)
		(drill oval 2.5 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -8.3 5.85)
		(size 3.8 1.4)
		(drill oval 2.5 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Connfly_DS1098_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
