(footprint "USB_A_Molex_105057_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.molex.com/pdm_docs/sd/1050570001_sd.pdf")
	(tags "USB A Vertical")
	(property "Reference" "REF**"
		(at 4.4 -7.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_Molex_105057_Vertical"
		(at 3.5 2.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.45 -2.15 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.3 1.3)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.3 1.3)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 4.5 0)
		(size 1.3 1.3)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7 0)
		(size 1.3 1.3)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -3.07 -0.6 180)
		(size 1.9 2.9)
		(drill oval 1.3 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 3.5 -4.78 90)
		(size 1.9 2.9)
		(drill oval 1.3 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 10.07 -0.6)
		(size 1.9 2.9)
		(drill oval 1.3 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_105057_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
