(footprint "USB_A_Receptacle_GCT_USB1046"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "GCT USB1046, USB Type A, https://gct.co/files/drawings/usb1046.pdf")
	(tags "USB SMD Type-A Receptacle Right Angle")
	(property "Reference" "REF**"
		(at 0 -10 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_Receptacle_GCT_USB1046"
		(at 0 8.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 4.97 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd oval
		(at -6.4 -3.55)
		(size 1.2 2.9)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
	)
	(pad "" smd oval
		(at 6.4 -3.55)
		(size 1.2 2.9)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -3.5 -7.25)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1 -7.25)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1 -7.25)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 3.5 -7.25)
		(size 1.3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" thru_hole oval
		(at -6.4 -3.55)
		(size 1.2 2.9)
		(drill oval 0.6 2.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "5" thru_hole oval
		(at 6.4 -3.55)
		(size 1.2 2.9)
		(drill oval 0.6 2.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Receptacle_GCT_USB1046.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
