(footprint "USB_A_Receptacle_XKB_U231-091N-4BLRA00-S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB 3.0 Type A, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2110100130_XKB-Connectivity-U231-091N-4BLRA00-S_C2880618.pdf")
	(tags "USB A Type-A Receptacle SMD")
	(property "Reference" "REF**"
		(at 0 -8.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_Receptacle_XKB_U231-091N-4BLRA00-S"
		(at 0 8.6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 -5.45 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 -5.45 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3.45 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 3 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 4 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -4 -6.4)
		(size 0.7 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" thru_hole oval
		(at -6.4 -5.25)
		(size 1.2 3.1)
		(drill oval 0.6 2.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" smd roundrect
		(at -6.4 0.95)
		(size 1.2 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" thru_hole oval
		(at 6.4 -5.25)
		(size 1.2 3.1)
		(drill oval 0.6 2.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" smd roundrect
		(at 6.4 0.95)
		(size 1.2 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Receptacle_XKB_U231-091N-4BLRA00-S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
