(footprint "USB_A_TE_292303-7_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB type A, Horizontal, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=292303&DocType=Customer+Drawing&DocLang=English")
	(tags "USB_A Female Connector receptacle")
	(property "Reference" "REF**"
		(at 0 -9.42 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_TE_292303-7_Horizontal"
		(at 0 9.09 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -1.71 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.5 -6.38)
		(size 1.25 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1 -6.38)
		(size 1.25 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1 -6.38)
		(size 1.25 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.5 -6.38)
		(size 1.25 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" thru_hole circle
		(at -6.57 -2.7)
		(size 3 3)
		(drill 2.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 6.57 -2.7)
		(size 3 3)
		(drill 2.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_TE_292303-7_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
