(footprint "USB_A_Wuerth_614004134726_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB A connector https://www.we-online.com/catalog/datasheet/614004134726.pdf")
	(tags "USB_A Female Connector receptacle")
	(property "Reference" "REF**"
		(at 0 -5.08 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_A_Wuerth_614004134726_Horizontal"
		(at 0 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.855 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2 0)
		(size 1.6 1.6)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 4 0)
		(size 1.6 1.6)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 6 0)
		(size 1.6 1.6)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -0.73 -2.72)
		(size 2.15 2.15)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -0.73 2.72)
		(size 2.15 2.15)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 6.27 -2.72)
		(size 2.15 2.15)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 6.27 2.72)
		(size 2.15 2.15)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Wuerth_614004134726_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
