(footprint "USB_C_Plug_JAE_DX07P024AJ1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, https://www.jae.com/en/searchfilter/?topics_keyword=DX07P024AJ1&mainItemSelect=1")
	(tags "USB Type-C Plug Edge Mount")
	(property "Reference" "REF**"
		(at -2.6925 -3.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Plug_JAE_DX07P024AJ1"
		(at -0.1725 4.27 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -4.3 -1.93)
		(end -4.3 -0.2275)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.3 -0.2275)
		(end -3.9 -0.2275)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.9 1.9225)
		(end -3.9 -0.2275)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.53 2.3725)
		(end -3.9 1.9225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.125 2.3725)
		(end -3.53 2.3725)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.925 2.8225)
		(end -2.925 2.5725)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.5 3.0225)
		(end -2.725 3.0225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.3 2.6225)
		(end -0.3 2.8225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.1 2.4225)
		(end 0.9 2.4225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.1 2.8225)
		(end 1.1 2.6225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.3 3.0225)
		(end 2.725 3.0225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.925 2.8225)
		(end 2.925 2.5725)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.125 2.3725)
		(end 3.575 2.3725)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.575 2.3725)
		(end 3.9 1.9225)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.9 1.9225)
		(end 3.9 -1.9175)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -3.125 2.3725)
		(mid -2.983579 2.431079)
		(end -2.925 2.5725)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.725 3.0225)
		(mid -2.866421 2.963921)
		(end -2.925 2.8225)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -0.3 2.6225)
		(mid -0.241421 2.481079)
		(end -0.1 2.4225)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -0.3 2.8225)
		(mid -0.358579 2.963921)
		(end -0.5 3.0225)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 0.9 2.4225)
		(mid 1.041421 2.481079)
		(end 1.1 2.6225)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 1.3 3.0225)
		(mid 1.158579 2.963921)
		(end 1.1 2.8225)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 2.925 2.5725)
		(mid 2.983579 2.431079)
		(end 3.125 2.3725)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 2.925 2.8225)
		(mid 2.866421 2.963921)
		(end 2.725 3.0225)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB Edge"
		(at 0 3.0225 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.5525 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.405 1.0475)
		(size 0.36 1.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "" smd rect
		(at 3.405 1.0475)
		(size 0.36 1.75)
		(layers "F.Cu" "F.Mask")
	)
	(pad "A1" smd rect
		(at 2.825 1.1475)
		(size 0.41 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at 2.25 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at 1.75 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at 1.25 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at 0.75 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at 0.25 1.1475 180)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at -0.25 1.1475 180)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at -0.75 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at -1.25 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at -1.75 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at -2.25 1.1475)
		(size 0.26 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at -2.825 1.1475)
		(size 0.41 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at -2.825 1.1475)
		(size 0.41 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B2" smd rect
		(at -2.25 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B3" smd rect
		(at -1.75 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B4" smd rect
		(at -1.25 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B5" smd rect
		(at -0.75 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B6" smd rect
		(at -0.25 1.1475 180)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B7" smd rect
		(at 0.25 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B8" smd rect
		(at 0.75 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B9" smd rect
		(at 1.25 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B10" smd rect
		(at 1.75 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B11" smd rect
		(at 2.25 1.1475)
		(size 0.26 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B12" smd rect
		(at 2.825 1.1475)
		(size 0.41 1.55)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "S1" smd rect
		(at -3.625 -1.1725)
		(size 0.8 1.5)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "S1" smd rect
		(at -3.405 0.8975)
		(size 0.36 2.05)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "S1" smd rect
		(at 3.27 -1.1725 180)
		(size 0.7 1.5)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "S1" smd rect
		(at 3.405 0.8975)
		(size 0.36 2.05)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Plug_JAE_DX07P024AJ1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
