(footprint "USB_C_Plug_Molex_105444"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Universal Serial Bus (USB) Shielded I/O Plug, Type C, Right Angle, Surface Mount, http://www.molex.com/pdm_docs/sd/1054440001_sd.pdf")
	(tags "USB Type-C Plug Edge Mount")
	(property "Reference" "REF**"
		(at 0 2.04 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Plug_Molex_105444"
		(at 0 -1.96 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 -0.96 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.04 0)
		(layer "F.Fab")
	)
	(pad "A1" smd rect
		(at -2.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -1.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -1.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -0.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 0.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 1.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 1.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 2.25 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 2.75 0.04)
		(size 0.38 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at 2.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B2" smd rect
		(at 2.25 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B3" smd rect
		(at 1.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B4" smd rect
		(at 1.25 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B5" smd rect
		(at 0.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B8" smd rect
		(at -0.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B9" smd rect
		(at -1.25 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B10" smd rect
		(at -1.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B11" smd rect
		(at -2.25 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B12" smd rect
		(at -2.75 0.04)
		(size 0.38 1)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "S1" smd rect
		(at -3.42 0.88)
		(size 0.7 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" smd rect
		(at 3.42 0.88)
		(size 0.7 1.15)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Plug_Molex_105444.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
