(footprint "USB_C_Plug_ShenzhenJingTuoJin_918-118A2021Y40002_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Low-profile vertical USB 2.0 Type C Plug Shenzhen Jing Tuo Jin Electronics Co 918-118A2021Y40002 ( https://datasheet.lcsc.com/lcsc/1912111437_Jing-Extension-of-the-Electronic-Co--918-118A2021Y40002_C399939.pdf ) also compatible with Korean HRO Parts Elec TYPE-C-31-G-06")
	(tags "type-c usb2")
	(property "Reference" "REF**"
		(at -2.6 -0.4 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Plug_ShenzhenJingTuoJin_918-118A2021Y40002_Vertical"
		(at 0.254 2.794 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "A1" smd roundrect
		(at -1.27 -2.8 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A4" smd roundrect
		(at -1.27 -2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A5" smd roundrect
		(at -1.27 -1.2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A6" smd roundrect
		(at -1.27 -0.4 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A7" smd roundrect
		(at -1.27 0.4 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A8" smd roundrect
		(at -1.27 1.2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A9" smd roundrect
		(at -1.27 2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A12" smd roundrect
		(at -1.27 2.8 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B1" smd roundrect
		(at 1.27 2.8 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B4" smd roundrect
		(at 1.27 2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B5" smd roundrect
		(at 1.27 1.2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B6" smd roundrect
		(at 1.27 0.4 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B7" smd roundrect
		(at 1.27 -0.4 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B8" smd roundrect
		(at 1.27 -1.2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B9" smd roundrect
		(at 1.27 -2 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B12" smd roundrect
		(at 1.27 -2.8 90)
		(size 0.4 0.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S1" smd roundrect
		(at 0 -3.95 90)
		(size 0.65 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S1" smd roundrect
		(at 0 3.95 90)
		(size 0.65 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Plug_ShenzhenJingTuoJin_918-118A2021Y40002_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
