(footprint "USB_C_Receptacle_Amphenol_12401548E4-2A_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB TYPE C, RA RCPT PCB, Hybrid, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401548E4%7e2A")
	(tags "USB C Type-C Receptacle Hybrid")
	(property "Reference" "REF**"
		(at 0 -6.36 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_Amphenol_12401548E4-2A_CircularHoles"
		(at 0 6.14 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.6 -4.36)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.6 -4.36)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd rect
		(at -2.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -1.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -1.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -0.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 0.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 1.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 1.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 2.25 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 2.75 -5.02)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" thru_hole circle
		(at 2.8 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B2" thru_hole circle
		(at 2.4 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B3" thru_hole circle
		(at 1.6 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at 1.2 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at 0.8 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at 0.4 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at -0.4 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at -0.8 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at -1.2 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B10" thru_hole circle
		(at -1.6 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B11" thru_hole circle
		(at -2.4 -3.01)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at -2.8 -3.71)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at -4.49 2.84)
		(size 1.4 1.4)
		(drill 1.1)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at -4.13 -3.11)
		(size 1.4 1.4)
		(drill 1.1)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at 4.13 -3.11)
		(size 1.4 1.4)
		(drill 1.1)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at 4.49 2.84)
		(size 1.4 1.4)
		(drill 1.1)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_12401548E4-2A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
