(footprint "USB_C_Receptacle_Amphenol_12401948E412A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB TYPE C, USB 2.0, SMT, https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/c12401948.pdf")
	(tags "Amphenol")
	(property "Reference" "REF**"
		(at 0 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_Amphenol_12401948E412A"
		(at 0 7.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -6.7 1.36)
		(end -4.57 1.36)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.57 -3)
		(end -4.57 1.36)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.42 -3.15)
		(end 4.42 -3.15)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.57 -3)
		(end 4.57 1.36)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.57 1.36)
		(end 6.7 1.36)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -4.57 -3)
		(mid -4.526066 -3.106066)
		(end -4.42 -3.15)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 4.42 -3.15)
		(mid 4.526066 -3.106066)
		(end 4.57 -3)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB EDGE"
		(at 3.25 2.25 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole oval
		(at -5.92 0)
		(size 0.9 1.8)
		(drill oval 0.6 1.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "" thru_hole oval
		(at -4.65 -4.32)
		(size 0.9 1.5)
		(drill oval 0.6 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "" np_thru_hole circle
		(at -3.5 -3.85)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.5 -3.85)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" thru_hole oval
		(at 4.65 -4.32)
		(size 0.9 1.5)
		(drill oval 0.6 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "" thru_hole oval
		(at 5.92 0)
		(size 0.9 1.8)
		(drill oval 0.6 1.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "A1" smd roundrect
		(at -3.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A4" smd roundrect
		(at -2.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A5" smd roundrect
		(at -1.25 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A6" smd roundrect
		(at -0.25 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A7" smd roundrect
		(at 0.25 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A8" smd roundrect
		(at 1.25 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A9" smd roundrect
		(at 2.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A12" smd roundrect
		(at 3.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B1" smd roundrect
		(at 3.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B4" smd roundrect
		(at 2.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B5" smd roundrect
		(at 1.75 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B6" smd roundrect
		(at 0.75 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B7" smd roundrect
		(at -0.75 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B8" smd roundrect
		(at -1.75 -5.1)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B9" smd roundrect
		(at -2.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B12" smd roundrect
		(at -3.5 -5.1)
		(size 0.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_12401948E412A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
