(footprint "USB_C_Receptacle_Amphenol_124019772112A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB TYPE C Receptacle, USB2.0, Waterproof, Dual Row SMT, IPX8, https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/c12401977-3.pdf")
	(tags "USB C Type-C Waterproof")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_Amphenol_124019772112A"
		(at 0 7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 1.575 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 1.575 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "Keep out zone"
		(at 0 5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "A1" smd roundrect
		(at -3.55 -3.2)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A1" smd roundrect
		(at -3.05 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A1" smd roundrect
		(at 3.55 -3.2)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A4" smd roundrect
		(at -1.25 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A5" smd roundrect
		(at -0.75 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A6" smd roundrect
		(at -0.25 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A7" smd roundrect
		(at 0.25 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A8" smd roundrect
		(at 0.75 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A9" smd roundrect
		(at 1.25 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A12" smd roundrect
		(at 3.05 -3.2)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B1" smd roundrect
		(at 3 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B4" smd roundrect
		(at 1.5 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B5" smd roundrect
		(at 1 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B6" smd roundrect
		(at 0.5 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B7" smd roundrect
		(at -0.5 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B8" smd roundrect
		(at -1 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B9" smd roundrect
		(at -1.5 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B12" smd roundrect
		(at -3 -1.95)
		(size 0.25 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "S1" thru_hole oval
		(at -4.45 -3.025)
		(size 0.95 1.95)
		(drill oval 0.45 1.45)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "S1" thru_hole oval
		(at -4.45 0.175)
		(size 0.95 2.15)
		(drill oval 0.45 1.65)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "S1" thru_hole oval
		(at 4.45 -3.025)
		(size 0.95 1.95)
		(drill oval 0.45 1.45)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(pad "S1" thru_hole oval
		(at 4.45 0.175)
		(size 0.95 2.15)
		(drill oval 0.45 1.65)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_124019772112A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
