(footprint "USB_C_Receptacle_CNCTech_C-ARA1-AK51X"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Type-C 3.0 Receptacle, 24-pin, right angle (source: https://www.cnctech.us/pdfs/C-ARA1-AK512.pdf)")
	(tags "USB C Type-C Receptacle Hybrid CNCTech C-ARA1-AK51X")
	(property "Reference" "REF**"
		(at 0 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_CNCTech_C-ARA1-AK51X"
		(at -0.02 7.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 4.84 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1 0)
		(layer "F.Fab")
	)
	(pad "A1" smd rect
		(at -2.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -2.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -1.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -1.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -0.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 0.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 1.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 1.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 2.25 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 2.75 -3.31)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" thru_hole circle
		(at 2.8 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B2" thru_hole circle
		(at 2.4 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B3" thru_hole circle
		(at 1.6 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at 1.2 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at 0.8 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at 0.4 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at -0.4 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at -0.8 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at -1.2 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B10" thru_hole circle
		(at -1.6 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B11" thru_hole circle
		(at -2.4 -1.3)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at -2.8 -2.2)
		(size 0.65 0.65)
		(drill 0.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -4.575 2)
		(size 0.95 2.28)
		(drill oval 0.55 1.6
			(offset 0 -0.14)
		)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -4.39 -1.05)
		(size 1.33 1.98)
		(drill oval 0.93 1.58)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -4.295 -3.03)
		(size 0.95 1.8)
		(drill oval 0.55 1.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" smd rect
		(at -3.375 -4.095)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" smd rect
		(at 3.375 -4.095)
		(size 0.7 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" thru_hole oval
		(at 4.295 -3.03)
		(size 0.95 1.8)
		(drill oval 0.55 1.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 4.39 -1.05)
		(size 1.33 1.98)
		(drill oval 0.93 1.58)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 4.575 2)
		(size 0.95 2.28)
		(drill oval 0.55 1.6
			(offset 0 -0.14)
		)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_CNCTech_C-ARA1-AK51X.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
