(footprint "USB_C_Receptacle_G-Switch_GT-USB-7025"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Type C, right-angle, SMT, https://www.lcsc.com/datasheet/lcsc_datasheet_2312191005_G-Switch-GT-USB-7025_C963213.pdf")
	(tags "USB C Type-C Receptacle SMD")
	(property "Reference" "REF**"
		(at 0 -4.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_G-Switch_GT-USB-7025"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 -1.65 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 -1.65 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 2.35 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.65 0)
		(layer "F.Fab")
	)
	(pad "A1" smd roundrect
		(at -3 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A4" smd roundrect
		(at -2.2 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A5" smd roundrect
		(at -1.4 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A6" smd roundrect
		(at -0.6 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A7" smd roundrect
		(at -0.2 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A8" smd roundrect
		(at 0.2 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A9" smd roundrect
		(at 1.8 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A12" smd roundrect
		(at 2.6 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B1" smd roundrect
		(at 3 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B4" smd roundrect
		(at 2.2 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B5" smd roundrect
		(at 1.4 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B6" smd roundrect
		(at 1 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B7" smd roundrect
		(at 0.6 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B8" smd roundrect
		(at -1 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B9" smd roundrect
		(at -1.8 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B12" smd roundrect
		(at -2.6 -3.45)
		(size 0.28 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "GND" smd roundrect
		(at -3.515 -3.45)
		(size 0.45 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "GND" smd roundrect
		(at 3.515 -3.45)
		(size 0.45 0.83)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S1" thru_hole circle
		(at -4.595 -2.69)
		(size 0.85 0.85)
		(drill 0.55)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -4.595 0.29)
		(size 0.55 2.05)
		(drill oval 0.25 1.75)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at 4.595 -2.69)
		(size 0.85 0.85)
		(drill 0.55)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 4.595 0.29)
		(size 0.55 2.05)
		(drill oval 0.25 1.75)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7025.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
