(footprint "USB_C_Receptacle_G-Switch_GT-USB-7051x"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Type C, vertical, SMT, https://datasheet.lcsc.com/lcsc/2108072030_G-Switch-GT-USB-7051A_C2843970.pdf")
	(tags "USB C Type-C Receptacle SMD GT-USB-7051A GT-USB-7051B")
	(property "Reference" "REF**"
		(at -2.5 -4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_G-Switch_GT-USB-7051x"
		(at 0 4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.75 0)
		(size 0.66 0.66)
		(drill 0.66)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole oval
		(at 3.75 0)
		(size 1 0.58)
		(drill oval 1 0.58)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "A1" smd roundrect
		(at -2.78 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A4" smd roundrect
		(at -1.99 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A5" smd roundrect
		(at -1.2 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A6" smd roundrect
		(at -0.41 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A7" smd roundrect
		(at 0.38 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A8" smd roundrect
		(at 1.17 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A9" smd roundrect
		(at 1.96 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "A12" smd roundrect
		(at 2.75 -0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B1" smd roundrect
		(at 2.75 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B4" smd roundrect
		(at 1.96 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B5" smd roundrect
		(at 1.17 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B6" smd roundrect
		(at 0.38 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B7" smd roundrect
		(at -0.41 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B8" smd roundrect
		(at -1.2 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B9" smd roundrect
		(at -1.99 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "B12" smd roundrect
		(at -2.78 0.76)
		(size 0.3 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "S1" thru_hole circle
		(at -2.4 -2.15)
		(size 1.1 1.1)
		(drill 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at -2.4 2.15)
		(size 1.1 1.1)
		(drill 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at 2.4 -2.15)
		(size 1.1 1.1)
		(drill 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole circle
		(at 2.4 2.15)
		(size 1.1 1.1)
		(drill 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask" "F.Paste")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "peg")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 0.8 -1.8) (xy -0.8 -1.8) (xy -0.8 -2.5) (xy 0.8 -2.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(name "peg")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 0.8 2.5) (xy -0.8 2.5) (xy -0.8 1.8) (xy 0.8 1.8)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_G-Switch_GT-USB-7051x.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
