(footprint "USB_C_Receptacle_GCT_USB4085"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
	(tags "USB Type-C Receptacle Through-hole Right angle")
	(property "Reference" "REF**"
		(at 2.975 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_GCT_USB4085"
		(at 2.975 9.925 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PCB Edge"
		(at 2.975 6.1 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 2.975 4.025 0)
		(layer "F.Fab")
	)
	(pad "A1" thru_hole circle
		(at 0 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A4" thru_hole circle
		(at 0.85 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A5" thru_hole circle
		(at 1.7 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A6" thru_hole circle
		(at 2.55 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A7" thru_hole circle
		(at 3.4 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A8" thru_hole circle
		(at 4.25 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A9" thru_hole circle
		(at 5.1 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A12" thru_hole circle
		(at 5.95 0)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B1" thru_hole circle
		(at 5.95 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at 5.1 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at 4.25 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at 3.4 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at 2.55 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at 1.7 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at 0.85 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at 0 1.35)
		(size 0.7 0.7)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -1.35 0.98)
		(size 0.9 2.4)
		(drill oval 0.6 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -1.35 4.36)
		(size 0.9 1.7)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 7.3 0.98)
		(size 0.9 2.4)
		(drill oval 0.6 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 7.3 4.36)
		(size 0.9 1.7)
		(drill oval 0.6 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4085.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
