(footprint "USB_C_Receptacle_GCT_USB4110"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A, https://gct.co/files/drawings/usb4110.pdf")
	(tags "USB 2.0 C Type-C Receptacle SMD 16P 16C USB4110-GF-A")
	(property "Reference" "REF**"
		(at 0 -5.015 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_GCT_USB4110"
		(at 0 5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 3.075 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.89 -2.605)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.89 -2.605)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "A1" smd roundrect
		(at -3.2 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A4" smd roundrect
		(at -2.4 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A5" smd roundrect
		(at -1.25 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A6" smd roundrect
		(at -0.25 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A7" smd roundrect
		(at 0.25 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A8" smd roundrect
		(at 1.25 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A9" smd roundrect
		(at 2.4 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "A12" smd roundrect
		(at 3.2 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B1" smd roundrect
		(at 3.2 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B4" smd roundrect
		(at 2.4 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B5" smd roundrect
		(at 1.75 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B6" smd roundrect
		(at 0.75 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B7" smd roundrect
		(at -0.75 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B8" smd roundrect
		(at -1.75 -3.68)
		(size 0.3 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B9" smd roundrect
		(at -2.4 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "B12" smd roundrect
		(at -3.2 -3.68)
		(size 0.6 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "S1" smd roundrect
		(at -5.11 -3.105)
		(size 2.18 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
	)
	(pad "S1" smd roundrect
		(at -5.11 0.825)
		(size 2.18 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
	)
	(pad "S1" smd roundrect
		(at 5.11 -3.105)
		(size 2.18 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
	)
	(pad "S1" smd roundrect
		(at 5.11 0.825)
		(size 2.18 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4110.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
