(footprint "USB_C_Receptacle_JAE_DX07S016JA1R1500"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB TYPE C, USB 2.0, SMT, https://www.jae.com/en/connectors/series/detail/product/id=91780")
	(tags "USB C Type-C Receptacle SMD USB 2.0")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_C_Receptacle_JAE_DX07S016JA1R1500"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3 -1.95)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" smd rect
		(at -1.4 1.15)
		(size 1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 1.4 1.15)
		(size 1 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" np_thru_hole oval
		(at 3 -1.95)
		(size 0.85 0.6)
		(drill oval 0.85 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "A1" smd rect
		(at -3.1 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -2.35 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at -1.75 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at -0.25 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 0.75 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 1.75 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 2.35 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 3.1 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at 3.1 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at 2.35 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd rect
		(at 1.25 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd rect
		(at 0.25 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd rect
		(at -0.75 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd rect
		(at -1.25 -3.05)
		(size 0.27 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd rect
		(at -2.35 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd rect
		(at -3.1 -3.05)
		(size 0.52 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" thru_hole oval
		(at -4.32 -2.675)
		(size 1.3 2.3)
		(drill oval 0.6 1.6)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at -4.32 1.15)
		(size 1.3 2.6)
		(drill oval 0.6 1.9)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 4.32 -2.675)
		(size 1.3 2.3)
		(drill oval 0.6 1.6)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S1" thru_hole oval
		(at 4.32 1.15)
		(size 1.3 2.6)
		(drill oval 0.6 1.9)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_JAE_DX07S016JA1R1500.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
