(footprint "USB_Micro-AB_Molex_47590-0001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro USB AB receptacle, right-angle inverted (https://www.molex.com/pdm_docs/sd/475900001_sd.pdf)")
	(tags "Micro AB USB SMD")
	(property "Reference" "REF**"
		(at 0 -5.15 180)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-AB_Molex_47590-0001"
		(at 0 3.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -3.75 1.1)
		(end -2.8 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.8 -0.475)
		(end -2.8 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.95 -0.475)
		(end -1.95 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.95 1.1)
		(end 1.95 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.95 -0.475)
		(end 1.95 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.8 -0.475)
		(end 2.8 1.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.8 1.1)
		(end 3.75 1.1)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.8 -0.475)
		(mid -2.375 -0.9)
		(end -1.95 -0.475)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 1.95 -0.475)
		(mid 2.375 -0.9)
		(end 2.8 -0.475)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB Edge"
		(at 0 1.1 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.55 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.5 -0.35)
		(size 0.3 0.85)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 3.5 -0.35)
		(size 0.3 0.85)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at 1.3 -3.025)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.65 -3.025)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0 -3.025)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.65 -3.025)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.3 -3.025)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" thru_hole oval
		(at -4.175 -0.35)
		(size 1 1.9)
		(drill oval 0.6 1.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at -3.7375 -0.35)
		(size 0.875 1.9)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" thru_hole oval
		(at -2.225 -3.35)
		(size 1.05 1.25)
		(drill oval 0.65 0.85)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd roundrect
		(at 0 -0.35)
		(size 2.9 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1315789474)
	)
	(pad "6" thru_hole oval
		(at 2.225 -3.35)
		(size 1.05 1.25)
		(drill oval 0.65 0.85)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at 3.7375 -0.35)
		(size 0.875 1.9)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" thru_hole oval
		(at 4.175 -0.35)
		(size 1 1.9)
		(drill oval 0.6 1.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-AB_Molex_47590-0001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
