(footprint "USB_Micro-B_Amphenol_10103594-0001LF_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
	(tags "USB USB_B USB_micro USB_OTG")
	(property "Reference" "REF**"
		(at 1.925 -3.365 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Amphenol_10103594-0001LF_Horizontal"
		(at -0.025 4.435 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB edge"
		(at -0.025 2.235 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -0.025 -0.015 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.325 -1.765 90)
		(size 1.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.675 -1.765 90)
		(size 1.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.025 -1.765 90)
		(size 1.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.625 -1.765 90)
		(size 1.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.275 -1.765 90)
		(size 1.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.975 -0.565)
		(size 1.825 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.875 -1.865)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.755 0.185)
		(size 1.35 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at -2.755 1.115 90)
		(size 1.7 1.35)
		(drill oval 1.2 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at -2.445 -1.885 90)
		(size 1.5 1.1)
		(drill oval 1.05 0.65)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at -0.985 1.385 90)
		(size 2.5 1.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.935 1.385 90)
		(size 2.5 1.43)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at 2.395 -1.885 90)
		(size 1.5 1.1)
		(drill oval 1.05 0.65)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 2.705 1.115 90)
		(size 1.7 1.35)
		(drill oval 1.2 0.7)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at 2.725 0.185)
		(size 1.35 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.875 -1.885)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.975 -0.565)
		(size 1.825 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10103594-0001LF_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
