(footprint "USB_Micro-B_Molex-105017-0001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
	(tags "Micro-USB SMD Typ-B")
	(property "Reference" "REF**"
		(at 0 -3.1125 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Molex-105017-0001"
		(at 0.3 4.3375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 2.6875 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.8875 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.3 -1.4625)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -1.4625)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -1.4625)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -1.4625)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -1.4625)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at -3.5 1.2375 180)
		(size 1.2 1.9)
		(drill oval 0.6 1.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at -2.9 1.2375)
		(size 1.2 1.9)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" thru_hole circle
		(at -2.5 -1.4625)
		(size 1.45 1.45)
		(drill 0.85)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at -1 1.2375)
		(size 1.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1 1.2375)
		(size 1.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole circle
		(at 2.5 -1.4625)
		(size 1.45 1.45)
		(drill 0.85)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at 2.9 1.2375)
		(size 1.2 1.9)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" thru_hole oval
		(at 3.5 1.2375)
		(size 1.2 1.9)
		(drill oval 0.6 1.3)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
