(footprint "USB_Micro-B_Molex-105133-0031"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Vertical Micro USB Typ-B (http://www.molex.com/pdm_docs/sd/1051330031_sd.pdf)")
	(tags "Micro-USB SMD Typ-B Vertical")
	(property "Reference" "REF**"
		(at 0 -2.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Molex-105133-0031"
		(at 0 3.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -0.375 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.3 -0.825)
		(size 0.45 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -0.825)
		(size 0.45 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -0.825)
		(size 0.45 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -0.825)
		(size 0.45 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -0.825)
		(size 0.45 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at -2.8 -1.075)
		(size 1.8 1.1)
		(drill oval 1.2 0.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 0 1.075)
		(size 2.2 1.1)
		(drill oval 1.6 0.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 2.8 -1.075)
		(size 1.8 1.1)
		(drill oval 1.2 0.5)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex-105133-0031.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
