(footprint "USB_Micro-B_Molex_47346-0001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
	(tags "Micro B USB SMD")
	(property "Reference" "REF**"
		(at 0 -3.3 180)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Molex_47346-0001"
		(at 0 4.6 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 2.67 180)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.2 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.3 -1.46)
		(size 0.45 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -1.46)
		(size 0.45 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -1.46)
		(size 0.45 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -1.46)
		(size 0.45 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -1.46)
		(size 0.45 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.375 1.2)
		(size 1.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.4875 -1.375)
		(size 1.425 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.15 1.2)
		(size 1.8 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.55 1.2)
		(size 1 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.4875 -1.375)
		(size 1.425 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3.375 1.2)
		(size 1.65 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
