(footprint "USB_Micro-B_Technik_TWP-4002D-H3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Dustproof Micro USB Type B TWP-4002D-H3, https://www.technik.com.hk/images/pdf_product/WP4002D-H3-A_2.0.pdf")
	(tags "USB Micro B horizontal dustproof waterproof IP67")
	(property "Reference" "REF**"
		(at 0 -2.825 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Technik_TWP-4002D-H3"
		(at 0 7.275 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 2.5 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.5 1.175)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.5 1.175)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.3 -1.075)
		(size 0.4 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -1.075)
		(size 0.4 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -1.075)
		(size 0.4 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -1.075)
		(size 0.4 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -1.075)
		(size 0.4 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at -2.55 -1.025)
		(size 1.6 1.1)
		(drill oval 1.1 0.6)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 2.55 -1.025)
		(size 1.6 1.1)
		(drill oval 1.1 0.6)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Technik_TWP-4002D-H3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
