(footprint "USB_Micro-B_Wuerth_629105150521_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
	(tags "usb micro receptacle")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_Wuerth_629105150521_CircularHoles"
		(at 0 5.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 3.75 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 1.05 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.5 -0.8)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.5 -0.8)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.3 -1.9)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -1.9)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -1.9)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -1.9)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -1.9)
		(size 0.45 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole circle
		(at -3.875 1.95)
		(size 1.8 1.8)
		(drill 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -3.725 -1.85)
		(size 2 2)
		(drill 1.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 3.725 -1.85)
		(size 2 2)
		(drill 1.4)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 3.875 1.95)
		(size 1.8 1.8)
		(drill 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_629105150521_CircularHoles.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
