(footprint "USB_Micro-B_XKB_U254-051T-4BH83-F1S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "XKB Connectivity, USB Micro-B, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2206091745_XKB-Connectivity-U254-051T-4BH83-F1S_C397452.pdf")
	(tags "USB Micro-B Receptacle SMD")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Micro-B_XKB_U254-051T-4BH83-F1S"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 1.5 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2 -1.96)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2 -1.96)
		(size 0.6 0.6)
		(drill 0.6)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.3 -2.285)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.65 -2.285)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -2.285)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -2.285)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -2.285)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd custom
		(at -3.1 -2.16)
		(size 1 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 0.8) (xy -1.05 0.8) (xy -1.05 -0.8) (xy 1.05 -0.8) (xy 1.05 -0.35) (xy 0.55 0) (xy 0.55 0.4)
					(xy 0.8 0.65)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" thru_hole oval
		(at -2.825 0.39)
		(size 1 1.7)
		(drill oval 0.5 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at -1.2 0.39)
		(size 1.9 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.2 0.39)
		(size 1.9 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole oval
		(at 2.825 0.39)
		(size 0.85 1.7)
		(drill oval 0.5 1.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd custom
		(at 3.1 -2.16)
		(size 1 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 0.8) (xy 1.05 0.8) (xy 1.05 -0.8) (xy -1.05 -0.8) (xy -1.05 -0.35) (xy -0.55 0) (xy -0.55 0.4)
					(xy -0.8 0.65)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_XKB_U254-051T-4BH83-F1S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
