(footprint "USB_Mini-B_AdamTech_MUSB-B5-S-VT-TSMT-1_SMD_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.adam-tech.com/upload/MUSB-B5-S-VT-TSMT-1.pdf")
	(tags "USB Mini-B")
	(property "Reference" "REF**"
		(at -2.18 4.39 90)
		(layer "F.SilkS")
	)
	(property "Value" "USB_Mini-B_AdamTech_MUSB-B5-S-VT-TSMT-1_SMD_Vertical"
		(at 0 7.58 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.49 0.015 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 1.85 -3 90)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.85 3 90)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.6 -1.6 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.6 -0.8 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.6 0 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.6 0.8 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.6 1.6 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.45 -4.75 90)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.45 4.75 90)
		(size 3 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Mini-B_AdamTech_MUSB-B5-S-VT-TSMT-1_SMD_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
