(footprint "DVI-I_Molex_74320-1004_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DVI-I Dual Link connector, horizontal, 29 pins, Molex P/N 74320-1004, https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/743/74320/743201004_sd.pdf?inline")
	(tags "dvi right angle")
	(property "Reference" "REF**"
		(at 9.525 -3.19 0)
		(layer "F.SilkS")
	)
	(property "Value" "DVI-I_Molex_74320-1004_Horizontal"
		(at 9.525 18 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 9.525 9.0424 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 9.525 9.0424 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PCB Edge"
		(at 24.892 12.446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 9.525 3.8608 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 7.112)
		(size 1.93 1.93)
		(drill 1.93)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 19.05 7.112)
		(size 1.93 1.93)
		(drill 1.93)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1923076923)
	)
	(pad "2" thru_hole circle
		(at 1.905 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.81 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.715 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 7.62 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 9.525 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 11.43 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 13.335 0)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 1.905 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 3.81 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 5.715 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 7.62 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 9.525 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 11.43 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 13.335 1.905)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 1.905 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 3.81 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 5.715 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 7.62 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 9.525 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 11.43 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 13.335 3.81)
		(size 1.3 1.3)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C1" thru_hole circle
		(at 16.51 0.635)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C2" thru_hole circle
		(at 19.05 0.635)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C3" thru_hole circle
		(at 16.51 3.175)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C4" thru_hole circle
		(at 19.05 3.175)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C5" thru_hole circle
		(at 17.78 -0.635)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C5" thru_hole circle
		(at 17.78 4.445)
		(size 1.3 1.3)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -5.842 3.81)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 24.892 3.81)
		(size 3.5 3.5)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/DVI-I_Molex_74320-1004_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
