(footprint "HDMI_A_Amphenol_10029449-x01xLF_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDMI Type A connector, Amphenol 10029449-001TLF 10029449-001RLF 10029449-101TLF 10029449-101RLF, Right Angle(https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10029449.pdf)")
	(tags "hdmi right angle")
	(property "Reference" "REF**"
		(at 0 -7.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI_A_Amphenol_10029449-x01xLF_Horizontal"
		(at 0 5.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 3.5 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 4.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 3.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -0.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -2.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -2.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.75 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -4.25 -5)
		(size 0.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole circle
		(at -7.85 0.9)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -7.25 -4)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 7.25 -4)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 7.85 0.9)
		(size 1.8 1.8)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/HDMI_A_Amphenol_10029449-x01xLF_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
