(footprint "HDMI_A_Contact_Technology_HDMI-19APL2_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDMI Contact Technology Type A http://www.contactswitch.com/en/download.aspx?id=1449")
	(tags "HDMI Contact Technology Type A")
	(property "Reference" "REF**"
		(at -0.01 -2.53 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI_A_Contact_Technology_HDMI-19APL2_Horizontal"
		(at 0 15.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 0 2.2 0)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -0.28 7.11 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "3" smd rect
		(at -3.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "5" smd rect
		(at -2.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "7" smd rect
		(at -1.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "9" smd rect
		(at -0.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "11" smd rect
		(at 0.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "13" smd rect
		(at 1.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "15" smd rect
		(at 2.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 3 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "17" smd rect
		(at 3.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 4 0)
		(size 0.5 2.8)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "19" smd rect
		(at 4.5 0)
		(size 0.5 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.775 0.1)
		(size 0.6 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.775 0.1)
		(size 0.6 2.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "SH" smd rect
		(at 6.775 0.1)
		(size 0.6 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 6.775 0.1)
		(size 0.6 2.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/HDMI_A_Contact_Technology_HDMI-19APL2_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
