(footprint "HDMI_A_Kycon_KDMIX-SL1-NS-WS-B15_VerticalRightAngle"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDMI, Type A, Kycon KDMIX-SL1-NS-WS-B15, Vertical Right Angle, http://www.kycon.com/Pub_Eng_Draw/KDMIX-SL1-NS-WS-B15.pdf")
	(tags "hdmi type a")
	(property "Reference" "REF**"
		(at 5.5 -6 180)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI_A_Kycon_KDMIX-SL1-NS-WS-B15_VerticalRightAngle"
		(at 0.5 14 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PCB Edge"
		(at 0.5 -8.5 180)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.5 4.90875 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1 -1.9 180)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.5 11.35 180)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.3125)
	)
	(pad "2" thru_hole circle
		(at 1 0.5775 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 1.155 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1 1.7325 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 2.31 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 1 2.8875 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 3.465 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 1 4.0425 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 4.62 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 1 5.1975 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0 5.775 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 1 6.3525 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 6.93 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 1 7.5075 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 0 8.085 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 1 8.6625 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 0 9.24 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 1 9.8175 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 0 10.395 180)
		(size 0.8 0.8)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.75 1.85 180)
		(size 1.4 3.2)
		(drill oval 0.9 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.75 11.35 180)
		(size 1.4 3.2)
		(drill oval 0.9 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.75 -0.75 180)
		(size 1.4 3.2)
		(drill oval 0.9 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.75 8.25 180)
		(size 1.4 3.2)
		(drill oval 0.9 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/HDMI_A_Kycon_KDMIX-SL1-NS-WS-B15_VerticalRightAngle.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
