(footprint "HDMI_A_Molex_208658-1001_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDMI Molex Type A https://www.molex.com/pdm_docs/sd/2086581001_sd.pdf")
	(tags "HDMI Molex Type A")
	(property "Reference" "REF**"
		(at 1.715 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI_A_Molex_208658-1001_Horizontal"
		(at 1.715 10 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB Edge"
		(at 5.715 0 90)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 1.715 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.285 -4.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.285 -4)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.285 -3.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.285 -3)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.285 -2.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.285 -2)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.285 -1.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.285 -1)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.285 -0.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.285 0)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.285 0.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.285 1)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.285 1.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.285 2)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.285 2.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.285 3)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -3.285 3.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -3.285 4)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -3.285 4.5)
		(size 2.6 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -2.525 -7.25)
		(size 3.3 1.5)
		(drill oval 2.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.525 7.25)
		(size 3.3 1.5)
		(drill oval 2.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.435 -7.25)
		(size 2.3 1.5)
		(drill oval 1.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.435 7.25)
		(size 2.3 1.5)
		(drill oval 1.7 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/HDMI_A_Molex_208658-1001_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
