(footprint "HDMI_Micro-D_Molex_46765-2x0x"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HDMI, Micro, Type D, THT/SMD hybrid, 0.4mm pitch, 19 ckt, right angle (http://www.molex.com/pdm_docs/sd/467651301_sd.pdf)")
	(tags "hdmi micro type d right angle tht smd hybrid ")
	(property "Reference" "REF**"
		(at 0 -6.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "HDMI_Micro-D_Molex_46765-2x0x"
		(at 0 3.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEPOUT"
		(at 0 -0.47 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 1.8 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.6 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.4 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.2 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.8 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.6 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.4 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.2 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.2 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -0.4 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -0.6 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -0.8 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -1.2 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.4 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.6 -3.55)
		(size 0.23 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.8 -4.775)
		(size 0.23 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -3.45 -3.36)
		(size 2.4 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole oval
		(at -3.1 0)
		(size 1.5 2.55)
		(drill oval 0.65 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 3.1 0)
		(size 1.5 2.55)
		(drill oval 0.65 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" smd rect
		(at 3.45 -3.36)
		(size 2.4 1.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -2.35 -2.64) (xy 2.35 -2.64) (xy 2.35 1.7) (xy -2.35 1.7)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Video.3dshapes/HDMI_Micro-D_Molex_46765-2x0x.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
